SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
2    PRODUCTS	3
2.1    Touch Screen User Interface	3
2.1.1    Basis of Design Touch Screen UI:	3
2.1.2    Device Architecture	3
2.1.3    Graphical Display	3
2.1.4    Touch UI Functions	4
2.1.5    Functions - The Touch Screen UI shall include:	4
2.1.6    Communication and Power	4
2.1.7    Physical	4
3    EXECUTION	5
4    APPENDICES	5
4.1    SPECIFIED PRODUCTS	5
4.1.1    Crestron TS-1542-C 	5
4.1.2    Crestron TS-1542-TILT 	5
4.1.3    Crestron TS-1542 	5
4.1.4    Crestron TS-1542-C-TILT 	5

1	GENERAL
NOT USED in this Guide Specification. Specifier shall Specify PART 1 administrative and procedural requirements as needed.
2	PRODUCTS

2.1	Touch Screen User Interface

2.1.1	Basis of Design Touch Screen UI:
Specifier Note: Please see system drawings or equipment lists for specified model and quantity.
2.1.1.1	Crestron TS-1542-C 

2.1.1.2	Crestron TS-1542-C-TILT 

2.1.1.3	Crestron TS-1542 

2.1.1.4	Crestron TS-1542-TILT 

2.1.1.5	Crestron TS-1542-C Signature Series  

2.1.2	Device Architecture

2.1.2.1	The Touch Screen UI shall be composed of the following functional elements: 

2.1.2.1.1	Graphical touch video display 

2.1.2.1.2	Programmable capacitive buttons 

2.1.2.1.3	Ambient light sensor 

2.1.2.1.4	Built-in microphone 

2.1.2.1.5	Built-in speakers 

2.1.2.1.6	Built-in Annotation Capability 

2.1.2.1.7	Built-In Single Cable Transmission Reciever
Specifier Note: The TS-1542-C and TS-1542-C-TILT include a DM input which includes Ethernet. DM matrix or transmitter must be connected to the required network for communication to the control processor. The TS-1542 and TS-1542-TILT include a LAN connectionwhich must be connected to the required network for communication to the control processor.
2.1.3	Graphical Display

2.1.3.1	Graphical UI - Touch screen UI display shall support the following viewable elements:

2.1.3.1.1	Control buttons and objects 

2.1.3.1.2	Feedback indication via text, button object change in color, animated object or graphical element. 

2.1.3.1.3	H.264 or MJPEG Streaming video 

2.1.3.1.4	Single Cable Transmission 4K Video 

2.1.3.1.5	HDCP 2.2  

2.1.3.2	Brightness Control - Graphical UI shall automatically adjust screen brightness based on room ambient light levels.  

2.1.4	Touch UI Functions

2.1.4.1	Touch Screen UI shall support Multi-Touch control interfacing. 

2.1.4.2	Touch Screen UI shall support gesture driven controls through custom programming and configuration.  

2.1.5	Functions - The Touch Screen UI shall include:

2.1.5.1	Custom Control UI - control of integrated system components through custom programming or preset configuration of the system control processor by same manufacturer. 

2.1.5.2	System Integration - device shall support controls for compatible integrated AV systems, HVAC and Lighting hardware, and  scheduling and management systems. 

2.1.5.3	Audio Intercom via Ethernet network.
Specifier Note: Intercom supports Crestron Rava enabled devices.
2.1.5.4	Built-in Annotation and Remote Annotation
Specifier Note: Remote Annotation requires additional compatible graphics engines.
2.1.5.5	Custom audio feedback via custom programming. 

2.1.5.6	Multi-Language support 

2.1.5.7	Internet Browsing shall be supported via Ethernet network.  
Specifier Note: Internet access required and to be provided by integrator.
2.1.5.8	Voice Recognition - device shall support voice commands control functionality through custom programming and configuratIon of the system control processor.
Specifier Note: Internet access required and to be provided by integrator.
2.1.6	Communication and Power

2.1.6.1	Communication: Bidirectional 10/100 Mbps Ethernet communication through the single cable transmission connection 

2.1.6.2	Power:  Power over DM or included power supply  

2.1.7	Physical

2.1.7.1	Touch Screen UI shall be available in the following sizes:

2.1.7.1.1	15.6 inch TFT active-matrix color LCD touch screen 1920 by 1080 resolution display.
Specifier Note: 5 inch version: Crestron TSW-560
3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS

4.1.1	Crestron TS-1542-C 

4.1.2	Crestron TS-1542-TILT 

4.1.3	Crestron TS-1542 

4.1.4	Crestron TS-1542-C-TILT