SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
1.1    SUMMARY	3
1.1.1    Section Includes	3
2    PRODUCTS	3
2.1    HD Multi-Window Processor	3
2.1.1    Basis of Design Product	3
2.1.2    Functions	3
2.1.3    Performance	4
3    EXECUTION	4
4    APPENDICES	4
4.1    SPECIFIED PRODUCTS	4
4.1.1    Crestron HD-WP-4K-401-C 	4

1	GENERAL

1.1	SUMMARY

1.1.1	Section Includes

1.1.1.1	HD Multi-Window Processor - A single unit integrated 4K multi-window processor and HDBaseT transmitter.     

2	PRODUCTS

2.1	HD Multi-Window Processor

2.1.1	Basis of Design Product

2.1.1.1	Crestron HD-WP-4K-401-C  

2.1.2	Functions

2.1.2.1	The HD Multi-Window Processor shall enable the display of up to four video sources simultaneously on a single HD, Ultra HD, or 4K display. 

2.1.2.2	The HD Multi-Window Processor shall support fully automatic basic operation without a control system. 

2.1.2.3	User control Interface

2.1.2.3.1	Front panel control 

2.1.2.3.2	Browser control 

2.1.2.3.3	Control System control  

2.1.2.4	Windowing modes supported:

2.1.2.4.1	Multi-Window 

2.1.2.4.2	Picture in Picture  

2.1.2.5	Text and Image Overlay

2.1.2.5.1	Custom text overlay for each window 

2.1.2.5.2	Custom text overlay at any screen location  

2.1.2.5.3	Custom photo or logo at any screen location   

2.1.3	Performance

2.1.3.1	The receiver shall meet the following minimum requirements:

2.1.3.1.1	HD digital video output:

2.1.3.1.1.1	One (1) 19-pin Type A HDMI female connector 

2.1.3.1.1.2	One (1) HDBaseT output  

2.1.3.1.2	The HD Multi-Window Processor shall include an HDBaseT output for support of 4K displays or receivers connected via HDBaseT.  

2.1.3.1.3	The HD Multi-Window Processor shall include an Ethernet port to interface with a control system by the same manufacturer. 

2.1.3.1.4	The HD Multi-Window Processor shall include built-in RS-232 and IR control ports to allow for programmable control of the connected devices via the control system.  

2.1.3.1.5	Supports HDCP 2.2. 

2.1.3.1.6	CEC device control.      

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS
Specifier Note: This Article includes Crestron products specified in this Guide Specification document. This Article is for reference only and should not be required in actual project manual unless included in an overall system equipment list. 
4.1.1	Crestron HD-WP-4K-401-C