SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
1.1    SUMMARY	3
1.1.1    Section Includes	3
2    PRODUCTS	3
2.1    HDBaseT RECEIVER AND GRAPHICS ENGINE	3
2.1.1    Basis of Design Graphics Engine HDBaseT receiver 	3
2.1.2    Functions	3
2.1.3    Performance	3
3    EXECUTION	4
4    APPENDICES	4
4.1    SPECIFIED PRODUCTS	4
4.1.1    Crestron DM-DGE-200-C 	4

1	GENERAL

1.1	SUMMARY

1.1.1	Section Includes

1.1.1.1	HDBaseT Receiver with Graphics Engine - A single unit integrated single cable transmission receiver and graphics engine processor with on-screen menu capability.     

2	PRODUCTS

2.1	HDBaseT RECEIVER AND GRAPHICS ENGINE

2.1.1	Basis of Design Graphics Engine HDBaseT receiver 

2.1.1.1	Crestron DM-DGE-200-C  

2.1.2	Functions

2.1.2.1	The Digital Graphics Engine adds touch screen controller capability to HD or Ultra HD touch screen displays. 

2.1.2.2	The Digital Graphics Engine with related software by same manufacturer supports the creation of a custom graphical user environment capable of combining controls of integrated equipment and systems with dual-window video display. 

2.1.2.3	The Digital Graphics Engine shall include an HDBaseT input for support of 4K UHD and DCI 4K sources connected at an HDBaseT transmitter or switcher.  

2.1.2.4	The Digital Graphics Engine shall support H.264 streaming video signals received over a high-speed Ethernet connection.  

2.1.2.5	The Digital Graphics Engine shall include an Ethernet port to interface with a control system by the same manufacturer. 

2.1.2.6	The Digital Graphics Engine shall include built-in RS-232 and IR control ports to allow for programmable control of the connected display and other devices via the control system.   

2.1.3	Performance

2.1.3.1	The receiver shall meet the following minimum requirements:

2.1.3.1.1	HDMI digital video, audio, and control output:

2.1.3.1.1.1	One (1) 19-pin Type A HDMI female connector  

2.1.3.1.2	HDMI output supports HDCP 2.2  

2.1.3.1.3	Streaming Decoder Video: 	H.264 (MPEG-4 part 10 AVC), MJPEG 

2.1.3.1.4	Supports HDCP. 

2.1.3.1.5	HDMI audio Support:  Up to 8 channel LPCM. 

2.1.3.1.6	CEC device control.      

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS
Specifier Note: This Article includes Crestron products specified in this Guide Specification document. This Article is for reference only and should not be required in actual project manual unless included in an overall system equipment list. 
4.1.1	Crestron DM-DGE-200-C