SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifer:  Please see PART 4 for a listing of products specified in this Guide Specification.

Table of Contents
1    GENERAL	3
1.1    SUMMARY	3
1.1.1    Section Includes	3
2    PRODUCTS	3
2.1    AV MULTI-FUNCTION PRESENTATION PROCESSOR	3
2.1.1    Basis of Design Product:	3
2.1.2    Device Architecture	3
2.1.3    Video System	3
2.1.4    Audio System	4
2.1.5    Single Cable Transmission System	5
2.1.6    Control Processor	5
2.1.7    Multimedia Presentation Gateway	6
3    EXECUTION	7
4    APPENDICES	7
4.1    SPECIFIED PRODUCTS	7
4.1.1    Crestron DMPS3-4K-200 	7
4.1.2    Crestron DMPS3-4K-300 	7
4.1.3    Crestron DMPS3-4K-250-C 	7
4.1.4    Crestron DMPS3-4K-350-C 	7

1	GENERAL

1.1	SUMMARY

1.1.1	Section Includes

1.1.1.1	AV Multi-Function Presentation System - A single unit integrated digital media presentation system.  The single central switching and control unit integrates audio-video switching, audio mixing and amplification, and system control.     

2	PRODUCTS

2.1	AV MULTI-FUNCTION PRESENTATION PROCESSOR

2.1.1	Basis of Design Product:

2.1.1.1	Crestron DMPS3-4K-[200/300/250/350]-C
SPECIFIER: See the following links for product selection: http://www.crestron.com/products/model/DMPS3-4K-200-C http://www.crestron.com/products/model/DMPS3-4K-300-C http://www.crestron.com/products/model/DMPS3-4K-250-C http://www.crestron.com/products/model/DMPS3-4K-350-C
2.1.2	Device Architecture

2.1.2.1	The Presentation Processor unit shall be a single unit composed of internally integrated components providing multiple functions.  Included sub-components:

2.1.2.1.1	Front Panel Control Interface shall provide basic control of the Presentation Processor. 

2.1.2.1.2	Audio Matrix/Mixer 

2.1.2.1.3	Audio Amplifier 

2.1.2.1.4	Video Matrix 

2.1.2.1.5	Single Cable Transmission 

2.1.2.1.6	Control Processor   

2.1.3	Video System

2.1.3.1	Video Inputs

2.1.3.1.1	Video inputs include HDMI and HDBaseT type input. 
SPECIFIER: the DMPS3-4K-200 includes INPUTS: (6) HDMI, (1) DM; OUTPUTS: (1) HDMI, (1) DM 
The DMPS3-4K-300/350 include INPUTS: (6) HDMI, (2) DM; OUTPUTS: (2) HDMI, (2) DM
2.1.3.1.1.1	HDBaseT type inputs shall be compatible with HDBaseT and manufacturers proprietary format supporting additional control functionality. 

2.1.3.1.1.2	HDMI inputs are compatible with DVI and Dual-Mode DisplayPort sources   

2.1.3.2	4K Video Switcher

2.1.3.2.1	Built-in video matrix switching allows video sources to be routed simultaneously to output connectors. 

2.1.3.2.2	Internal switcher shall support routing of HDMI and other AV sources to HDMI and HDBaseT outputs.
SPECIFIER: the DMPS3-4K-200/250 includes (1) HDMI and (1) DM output, the DMPS3-4K-300/350 include (2) HDMI and (2) DM outputs, 
2.1.3.2.3	The HDMI outputs are compatible with DVI and the HDBaseT outputs are compatible with HDBaseT and manufacturer proprietary format supporting additional control functionality. 

2.1.3.2.4	4K/60 Video Scaling - Unit shall include an independent, 4K scaler on each HDMI output.   

2.1.4	Audio System

2.1.4.1	Audio Inputs - Each HDMI and analog audio input includes adjustable input compensation to accommodate a range of signals and maintain consistent volume levels when switching between sources. 

2.1.4.2	Audio Amplifier - Unit shall include a built-in power amplifier.

2.1.4.2.1	Amplifier shall support three mutually exclusive amplifier modes. 

2.1.4.2.1.1	100V mode: mono, 40 Watts RMS per channel. 

2.1.4.2.1.2	4 ohm, 8 ohm mode: Stereo, 20 Watts RMS per channel at 4 ohms or 8 ohms. 

2.1.4.2.1.3	70V mode: mono, 40 Watts RMS per channel.   

2.1.4.3	Audio Matrix Functions:

2.1.4.3.1	Any analog input, digital audio input, or HDBaseT audio input signal shall be routable to:

2.1.4.3.1.1	Amplified Speaker Output 

2.1.4.3.1.2	Analog line level outputs 

2.1.4.3.1.3	HDBaseT type output 

2.1.4.3.1.4	HDMI output   

2.1.4.4	Microphone Preamplifier

2.1.4.4.1	Microphone Inputs - Each internal microphone preamplifier input shall be connected to two mutually exclusive input connections:

2.1.4.4.1.1	Detachable terminal block - Balanced microphone level analog audio with switchable 48 volt DC phantom power. 

2.1.4.4.1.2	Detachable terminal block - Balanced or unbalanced line level analog audio.   

2.1.4.5	Audio Mixer

2.1.4.5.1	All stereo audio outputs shall be capable of outputting independent microphone and program audio mixes.

2.1.4.5.1.1	All stereo sources and microphone sources shall be available simultaneously. 

2.1.4.5.1.2	All stereo sources and microphone sources shall have controllable levels in mixed output signal.   

2.1.4.6	Audio DSP

2.1.4.6.1	Each analog audio output shall include DSP processing, allowing each output to be configured separately.  DSP parameters include: 

2.1.4.6.1.1	real-time adjustable volume, bass, treble, and mute controls 

2.1.4.6.1.2	10-band graphic equalization 

2.1.4.6.1.3	4-band parametric equalization 

2.1.4.6.1.4	Adjustable limiting 

2.1.4.6.1.5	Up to 85 ms of speaker delay adjustment    

2.1.5	Single Cable Transmission System

2.1.5.1	HDBaseT type inputs and outputs allow for connecting to remote sources and display devices, and integrating with larger systems via a single CAT5 type cable. 

2.1.5.2	The one-wire interface supports transmission of ultra high-definition video, audio, control, power, and networking signals over CAT type cable at distances up to 330 feet (100 meters).  

2.1.5.3	Unit shall be HDBaseT Certified

2.1.5.3.1	The processor shall be designed using HDBaseT Alliance specifications, and shall support interoperability with other HDBaseT certified products.    

2.1.6	Control Processor

2.1.6.1	Unit shall include a built-in control processor with onboard control ports for control of external devices.

2.1.6.3	The Central Switching And Control Unit shall include an integrated microprocessor based control processor. 

2.1.6.4	The built-in control processor shall support customizable control of integrated AV devices, room lighting hardware, window shades, and projection screens. 

2.1.6.5	Controller shall include the following onboard control ports: 

2.1.6.6	Ethernet 

2.1.6.7	Four IR ports 

2.1.6.8	Two RS-232 COM ports 

2.1.6.9	Four relay ports 

2.1.6.10	Four digital input ports 

2.1.6.11	RS-422 type network control bus 

2.1.6.12	Control Subnet Networking
Specifier Note: Control subnet port and functionality is included in the DMPS3-4K-250-C and DMPS3-4K-350-C only.
2.1.6.12.1	Unit shall include a built-in control subnet network port.

2.1.6.13	The controller shall support a network management system by the same manufacturer, supporting overall remote system controlling, monitoring, and managing through network computers and mobile devices. 

2.1.6.14	The controller shall support touch screens, keypads, and wireless remotes and mobile device Apps from the same manufacturer.  

2.1.7	Multimedia Presentation Gateway
Specifier Note: AirMedia Gateway functionality is included in the DMPS3-4K-250-C and DMPS3-4K-350-C only.
2.1.7.1	General Functionality

2.1.7.1.1	Gateway shall support presentation of content from network connected devices.  

2.1.7.2	Architecture

2.1.7.2.1	Gateway functionality shall be a built-in function.  

2.1.7.3	Communication

2.1.7.3.1	Dedicated LAN Connection

2.1.7.3.1.1	10/100 Mbps, auto-switching, auto-negotiating, full/half duplex, DHCP, SSL, TLS, SSH, SNMP, IPv4, HTTPS web server   

2.1.7.4	User Device Support

2.1.7.4.1	Gateway shall support connection of up to 32 user devices for presentation. 

2.1.7.4.2	Gateway shall support multiple user device types and Operating Systems:

2.1.7.4.2.1	Laptop and desktop computers:

2.1.7.4.2.1.1	Windows XP, Windows Vista, Windows 7, Windows 8, Window 10, Mac OS X (versions 10.5 thru 10.11)  

2.1.7.4.2.2	Mobile Devices:

2.1.7.4.2.2.1	Apple iOS, Android    

2.1.7.5	Audio

2.1.7.5.1	Audio Format: Stereo  

2.1.7.6	Video

2.1.7.6.1	Video Frame Rate Supported: 15 fps (typical) 

2.1.7.6.2	Supported Resolutions

2.1.7.6.2.1	800x600@60Hz, 1024x768@60Hz, 1280x720@60Hz (720p60), 1280x768@60Hz, 1280x800@60Hz, 1280x1024@60Hz, 1360x768@60Hz, 1400x1050@60Hz, 1440x900@60Hz, 1600x1200@60Hz, 1920x1080@60Hz (1080p60), 1920x1200@60Hz       

3	EXECUTION
NOT USED in this Guide Specification. Specifier shall Specify PART 3 On-Site work as needed.
4	APPENDICES

4.1	SPECIFIED PRODUCTS

4.1.1	Crestron DMPS3-4K-200 

4.1.2	Crestron DMPS3-4K-300 

4.1.3	Crestron DMPS3-4K-250-C 

4.1.4	Crestron DMPS3-4K-350-C