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SECTION 27 41 16 
INTEGRATED AUDIO-VIDEO SYSTEMS AND EQUIPMENT 

GUIDE SPECIFICATION

Specifier: The Specifier/Design Professional is responsible for the accuracy of all project specifications, including system application and coordination with related sections.  This guide specification is provided as a convenience and requires editing to match actual project requirements.  CRESTRON ELECTRONICS, INC. SHALL NOT BE LIABLE FOR ANY DAMAGES ARISING OUT OF THE USE OF ANY OF ITS GUIDE SPECIFICATIONS.  For Crestron design assistance and design review please contact Sales Support Services Department at   800.237.2041 or techsales@crestron.com.

Specifier: Please see PART 4 for a listing of products specified in this Guide Specification.
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NOT USED in this Guide Specification.  Specifier shall Specify PART 1 administrative and procedural requirements as needed.


[bookmark: PRODUCTS][bookmark: BKM_66A60F3A_F8C2_4849_9125_C67075DA7144][bookmark: _Toc239857821]PRODUCTS



1.1 [bookmark: _Toc239857822]Room Availability Status Indicator, Wall Mount with USB-C Adapter

Specifier Note:
The SIW-100-USB KIT includes the SIW-100 room availability status indicator and the ADPT-USB-USB-RA USB-C® to USB-A adapter. Each adapter can be used to convert an existing room availability sign (SIW, SSW, or SSC series) from USB-A to USB-C for compatibility with TSW-80 touch screens.

1.1.1 [bookmark: _Toc239857823]Basis of Design

1.1.1.1 Crestron SIW-100-USB

Specifier Note:
SIW-100-USB
https://www.crestron.com/Products/Catalog/Scheduling/Availability-Signs/Wall-Mount/SIW-100-USB-KIT

[bookmark: _Toc239857824]Device Definition

Room Availability Status Indicator with the following capabilities and features:

Indication of room availability

Inclusion of USB-C® to USB-A adapter

Compatibility with touch screens by same manufacturer

Visibility at 50 ft (15 m)

Custom functionality when connected to control system by same manufacturer

Support for mounting in single-gang electrical box or plaster ring

Illumination in green or red to indicate room availability status

1.1.2 [bookmark: _Toc239857825]Device Architecture

Environmental

Temperature: 41° to 113°F (5° to 45° C)

Humidity: 10% to 90% RH (noncondensing)

Heat Dissipation

4 BTU/hr on USB power

7 BTU/hr on proprietary power/data transmission standard by same manufacturer

Construction

Composition: Metal bracket with replaceable acrylic lens and magnetically held gray plastic bezel

Mounting: Mounts to a 1-gang U.S. electrical box or plaster ring

Dimensions

Height: 6.41 in. (163 mm)

Width: 2.79 in. (71 mm)

Depth: 2.16 in. (55 mm)

USB-C to USB-A adapter length: 6.00 in. (152 mm)

Specifier Note:
Indicator projects 2 in. (52 mm) from the mounting surface

[bookmark: _Toc239857826]Functions

Indicator

Material: Acrylic

Illumination: Edge lit RGB LED

Functionality: Supports alternating red/green indication of room availability status when connected to a room scheduling touch screen via USB, supports RGB color mixing when connected to a control system

Communications

USB: USB 2.0 device for connection to touch screen by same manufacturer

Proprietary power/data transmission standard by same manufacturer: Network client mode

Connectors

USB

(1) Micro USB Type B connector, female

USB 2.0 device port

Plenum-rated 15 ft (4.57 m) micro B male to A male USB cable included

Controls

CNET ID: (1) Push button (behind bezel) for touch-settable ID utilizing proprietary power/data transmission standard by same manufacturer

Power

USB: 2.4 W @ 5 V USB power

Proprietary power/data transmission standard power usage: 2.4 W @ 24 VDC
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NOT USED in this Guide Specification.  Specifier shall Specify PART 3 On-Site work as needed.  
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Specifier Note: This Article includes Crestron products specified in this Guide Specification document.  This Article is for reference only and should not be required in actual project manual unless included in an overall system equipment list.  
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