## camerabin camerabin — Handle lot of features present in DSC |

## Synopsis

    struct              GstCameraBin;
    enum                GstCameraBinMode;

## Object Hierarchy

      GObject
       +----GstObject
             +----GstElement
                   +----GstBin
                         +----GstPipeline
                               +----GstCameraBin

## Implemented Interfaces

GstCameraBin implements GstChildProxy, GstImplementsInterface, GstColorBalance and GstTagSetter.

## Properties

      "audioenc"                 GstElement*           : Read / Write
      "audiosrc"                 GstElement*           : Read / Write
      "filename"                 gchar*                : Read / Write
      "filter-caps"              GstCaps*              : Read / Write
      "imageenc"                 GstElement*           : Read / Write
      "imagepp"                  GstElement*           : Read / Write
      "inputcaps"                GstCaps*              : Read
      "mode"                     GstCameraBinMode      : Read / Write
      "mute"                     gboolean              : Read / Write
      "vfsink"                   GstElement*           : Read / Write
      "videoenc"                 GstElement*           : Read / Write
      "videomux"                 GstElement*           : Read / Write
      "videopp"                  GstElement*           : Read / Write
      "videosrc"                 GstElement*           : Read / Write
      "zoom"                     gfloat                : Read / Write
      "preview-caps"             GstCaps*              : Read / Write
      "audio-encoder"            GstElement*           : Read / Write
      "audio-source"             GstElement*           : Read / Write
      "image-encoder"            GstElement*           : Read / Write
      "image-post-processing"    GstElement*           : Read / Write
      "video-encoder"            GstElement*           : Read / Write
      "video-muxer"              GstElement*           : Read / Write
      "video-post-processing"    GstElement*           : Read / Write
      "video-source"             GstElement*           : Read / Write
      "video-source-caps"        GstCaps*              : Read
      "viewfinder-sink"          GstElement*           : Read / Write
      "flags"                    GstCameraBinFlags     : Read / Write
      "block-after-capture"      gboolean              : Read / Write
      "image-capture-height"     gint                  : Read / Write
      "image-capture-width"      gint                  : Read / Write
      "video-capture-framerate"  GstFraction           : Read / Write
      "video-capture-height"     gint                  : Read / Write
      "video-capture-width"      gint                  : Read / Write
      "video-source-filter"      GstElement*           : Read / Write
      "viewfinder-filter"        GstElement*           : Read / Write
      "idle"                     gboolean              : Read
      "preview-source-filter"    GstElement*           : Read / Write
      "ready-for-capture"        gboolean              : Read

## Signals

      "img-done"                                       : Run Last
      "user-image-res"                                 : Action
      "user-pause"                                     : Action
      "user-res-fps"                                   : Action
      "user-start"                                     : Action
      "user-stop"                                      : Action
      "capture-pause"                                  : Action
      "capture-start"                                  : Action
      "capture-stop"                                   : Action
      "image-done"                                     : Run Last
      "set-image-resolution"                           : Action
      "set-video-resolution-fps"                       : Action

## Description

GstCameraBin is a high-level camera object that encapsulates the gstreamer internals and provides a task based API for the application. It consists of three main data paths: view-finder, image capture and video capture.

Structural decomposition of CameraBin object.

### Example launch line

    1
    gst-launch -v -m camerabin

### Image capture

Image capture is selected by switching "mode" to `MODE_IMAGE`. Taking still images is initiated with the "capture-start" action signal. Once the image has been captured, "image-captured" gst message is posted to the bus and capturing another image is possible. If application has set "preview-caps" property, then a "preview-image" gst message is posted to bus containing preview image formatted according to specified caps. Eventually when image has been saved "image-done" signal is emitted.

Available resolutions can be taken from the "video-source-caps" property. Image capture resolution can be set with "set-image-resolution" action signal.

Some video source elements implement the GstPhotography interface, which contains functions and properties for setting photography parameters. One can use `gst_bin_iterate_all_by_interface()` to get a reference to it.

### Video capture

Video capture is selected by switching "mode" to `MODE_VIDEO`. The capture is started with the "capture-start" action signal too. In addition to image capture one can use "capture-pause" to pause recording and "capture-stop" to end recording.

Available resolutions and fps can be taken from the "video-source-caps" property. "set-video-resolution-fps" action signal can be used to set frame rate and resolution for the video recording and view finder as well.

### States

Elements within GstCameraBin are created and destroyed when switching between NULL and READY states. Therefore element properties should be set in NULL state. User set elements are not unreffed until GstCameraBin is unreffed or replaced by a new user set element. Initially only elements needed for view finder mode are created to speed up startup. Image bin and video bin elements are created when setting the mode or starting capture.

### Video and image previews

GstCameraBin contains "preview-caps" property, which is used to determine whether the application wants a preview image of the captured picture or video. When set, a GstMessage named "preview-image" will be sent. This message will contain a GstBuffer holding the preview image, converted to a format defined by those preview caps. The ownership of the preview image is kept in GstCameraBin, so application should ref the preview buffer object if it needs to use it elsewhere than in message handler.

Defining preview caps is done by selecting the capturing "mode" first and then setting the property. Camerabin remembers caps separately for both modes, so it is not necessary to set the caps again after changing the mode.

### Note

Since the muxers tested so far have problems with discontinous buffers, QoS has been disabled, and then in order to record video, you MUST ensure that there is enough CPU to encode the video. Thus choose smart resolution and frames per second values. It is also highly recommended to avoid color conversions; make sure all the elements involved work with the same colorspace (i.e. rgb or yuv i420 or whatelse).

## Synopsis

### Element Information

plugin | camerabin
author | Nokia Corporation <multimedia@maemo.org>, Edgard Lima <edgard.lima@indt.org.br>
class | Generic/Bin/Camera

### Element Pads

## Details

### struct GstCameraBin

    struct GstCameraBin;

The opaque GstCameraBin structure.

### enum GstCameraBinMode

    typedef enum
    {
      MODE_IMAGE = 0,
      MODE_VIDEO
    } GstCameraBinMode;

Capture mode to use.

`MODE_IMAGE` | image capture
`MODE_VIDEO` | video capture

## Property Details

### The `"audioenc"` property

      "audioenc"                 GstElement*           : Read / Write

Audio encoder GStreamer element (default is vorbisenc).

### The `"audiosrc"` property

      "audiosrc"                 GstElement*           : Read / Write

Audio source GStreamer element (default is pulsesrc).

### The `"filename"` property

      "filename"                 gchar*                : Read / Write

Set filename for the still image capturing or video capturing.

Default value: ""

### The `"filter-caps"` property

      "filter-caps"              GstCaps*              : Read / Write

Caps applied to capsfilter element after videosrc [ ! ffmpegcsp ]. You can use this e.g. to make sure video color format matches with encoders and other elements configured to camerabin and/or change resolution and frame rate.

### The `"imageenc"` property

      "imageenc"                 GstElement*           : Read / Write

Image encoder GStreamer element (default is jpegenc).

### The `"imagepp"` property

      "imagepp"                  GstElement*           : Read / Write

Image Post-Processing GStreamer element (default is NULL).

### The `"inputcaps"` property

      "inputcaps"                GstCaps*              : Read

The allowed modes of the video source operation.

### The `"mode"` property

      "mode"                     GstCameraBinMode      : Read / Write

Set the mode of operation: still image capturing or video recording. Setting the mode will create and destroy image bin or video bin elements according to the mode. You can set this property at any time, changing the mode will stop ongoing capture.

Default value: Still image capture (default)

### The `"mute"` property

      "mute"                     gboolean              : Read / Write

Mute audio in video recording mode. Set this property only when GstCameraBin is in READY, PAUSED or PLAYING.

Default value: FALSE

### The `"vfsink"` property

      "vfsink"                   GstElement*           : Read / Write

View finder sink GStreamer element (default is autovideosink).

### The `"videoenc"` property

      "videoenc"                 GstElement*           : Read / Write

Video encoder GStreamer element (default is theoraenc).

### The `"videomux"` property

      "videomux"                 GstElement*           : Read / Write

Video muxer GStreamer element (default is oggmux).

### The `"videopp"` property

      "videopp"                  GstElement*           : Read / Write

Video post processing GStreamer element (default is NULL).

### The `"videosrc"` property

      "videosrc"                 GstElement*           : Read / Write

Video source GStreamer element (default is v4l2src).

### The `"zoom"` property

      "zoom"                     gfloat                : Read / Write

Set up the zoom applied to the frames. Set this property only when GstCameraBin is in READY, PAUSED or PLAYING.

Allowed values: [1,10]

Default value: 1

### The `"preview-caps"` property

      "preview-caps"             GstCaps*              : Read / Write

If application wants to receive a preview image, it needs to set this property to depict the desired image format caps. When this property is not set (NULL), message containing the preview image is not sent.

### The `"audio-encoder"` property

      "audio-encoder"            GstElement*           : Read / Write

Set up an audio encoder element. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"audio-source"` property

      "audio-source"             GstElement*           : Read / Write

Set up an audio source element. By default "autoaudiosrc" or DEFAULT_AUDIOSRC will be used. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"image-encoder"` property

      "image-encoder"            GstElement*           : Read / Write

Set up an image encoder (for example, jpegenc or pngenc) element. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"image-post-processing"` property

      "image-post-processing"    GstElement*           : Read / Write

Set up an element to do image post processing. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"video-encoder"` property

      "video-encoder"            GstElement*           : Read / Write

Set up a video encoder element. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"video-muxer"` property

      "video-muxer"              GstElement*           : Read / Write

Set up a video muxer element. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"video-post-processing"` property

      "video-post-processing"    GstElement*           : Read / Write

Set up an element to do video post processing. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"video-source"` property

      "video-source"             GstElement*           : Read / Write

Set up a video source element. By default "autovideosrc" or DEFAULT_VIDEOSRC will be used. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"video-source-caps"` property

      "video-source-caps"        GstCaps*              : Read

The allowed modes of operation of the video source. Have in mind that it doesn't mean GstCameraBin can operate in all those modes, it depends also on the other elements in the pipeline. Remember to gst_caps_unref after using it.

### The `"viewfinder-sink"` property

      "viewfinder-sink"          GstElement*           : Read / Write

Set up a sink element to render frames in view finder. By default "autovideosink" or DEFAULT_VIDEOSINK will be used. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"flags"` property

      "flags"                    GstCameraBinFlags     : Read / Write

Control the behaviour of camerabin.

Default value: Enable source crop and scale|Enable scale for viewfinder|Enable audio conversion for video capture|Enable colorspace conversion for still image|Enable colorspace conversion for video capture

### The `"block-after-capture"` property

      "block-after-capture"      gboolean              : Read / Write

Block viewfinder after capture. If it is TRUE when 'capture-start' is issued, camerabin will prepare to block and freeze the viewfinder after capturing. Setting it to FALSE will abort the blocking if it hasn't happened yet, or will enable again the viewfinder if it is already blocked. Note that setting this property to TRUE after 'capture-start' will only work for the next capture. This makes possible for applications to set the property to FALSE to abort the current blocking and already set it back to TRUE again to block at the next capture.

This is useful if application wants to display the preview image and running the viewfinder at the same time would be just a waste of CPU cycles.

Default value: FALSE

### The `"image-capture-height"` property

      "image-capture-height"     gint                  : Read / Write

The height to be used when capturing still images. If 0, the viewfinder's height will be used.

Allowed values: [0,32767]

Default value: 600

### The `"image-capture-width"` property

      "image-capture-width"      gint                  : Read / Write

The width to be used when capturing still images. If 0, the viewfinder's width will be used.

Allowed values: [0,32767]

Default value: 800

### The `"video-capture-framerate"` property

      "video-capture-framerate"  GstFraction           : Read / Write

The framerate to be used when capturing video.

### The `"video-capture-height"` property

      "video-capture-height"     gint                  : Read / Write

The height to be used when capturing video.

Allowed values: [0,32767]

Default value: 600

### The `"video-capture-width"` property

      "video-capture-width"      gint                  : Read / Write

The width to be used when capturing video.

Allowed values: [0,32767]

Default value: 800

### The `"video-source-filter"` property

      "video-source-filter"      GstElement*           : Read / Write

Set up optional video filter element, all frames from video source will be processed by this element. e.g. An application might add image enhancers/parameter adjustment filters here to improve captured image/video results, or add analyzers to give feedback on capture the application. This property can only be set while GstCameraBin is in NULL state. The ownership of the element will be taken by GstCameraBin.

### The `"viewfinder-filter"` property

      "viewfinder-filter"        GstElement*           : Read / Write

viewfinder filter GStreamer element.

### The `"idle"` property

      "idle"                     gboolean              : Read

When TRUE no capturing/encoding/saving is running and it is safe to set camerabin to NULL to release resources without losing data.

In case of errors, this property is made unreliable. Set the pipeline back to READY or NULL to make it reliable again.

Default value: TRUE

### The `"preview-source-filter"` property

      "preview-source-filter"    GstElement*           : Read / Write

Optional preview source filter GStreamer element.

### The `"ready-for-capture"` property

      "ready-for-capture"        gboolean              : Read

When TRUE new capture can be prepared. If FALSE capturing is ongoing and starting a new capture immediately is not possible.

Default value: TRUE

## Signal Details

### The `"img-done"` signal

    gboolean            user_function                      (GstCameraBin *gstcamerabin,
                                                            gchar        *arg1,
                                                            gpointer      user_data)         : Run Last

`gstcamerabin` : | the object which received the signal.
`user_data` : | user data set when the signal handler was connected.

### The `"user-image-res"` signal

    void                user_function                      (GstCameraBin *gstcamerabin,
                                                            gint          arg1,
                                                            gint          arg2,
                                                            gpointer      user_data)         : Action

`gstcamerabin` : | the object which received the signal.
`user_data` : | user data set when the signal handler was connected.

### The `"user-pause"` signal

    void                user_function                      (GstCameraBin *gstcamerabin,
                                                            gpointer      user_data)         : Action

`gstcamerabin` : | the object which received the signal.
`user_data` : | user data set when the signal handler was connected.

### The `"user-res-fps"` signal

    void                user_function                      (GstCameraBin *gstcamerabin,
                                                            gint          arg1,
                                                            gint          arg2,
                                                            gint          arg3,
                                                            gint          arg4,
                                                            gpointer      user_data)         : Action

`gstcamerabin` : | the object which received the signal.
`user_data` : | user data set when the signal handler was connected.

### The `"user-start"` signal

    void                user_function                      (GstCameraBin *gstcamerabin,
                                                            gpointer      user_data)         : Action

`gstcamerabin` : | the object which received the signal.
`user_data` : | user data set when the signal handler was connected.

### The `"user-stop"` signal

    void                user_function                      (GstCameraBin *gstcamerabin,
                                                            gpointer      user_data)         : Action

`gstcamerabin` : | the object which received the signal.
`user_data` : | user data set when the signal handler was connected.

### The `"capture-pause"` signal

    void                user_function                      (GstCameraBin *camera,
                                                            gpointer      user_data)      : Action

Pauses video recording or resumes paused video recording. If in image mode or not recording, does nothing.

`camera` : | the camera bin element
`user_data` : | user data set when the signal handler was connected.

### The `"capture-start"` signal

    void                user_function                      (GstCameraBin *camera,
                                                            gpointer      user_data)      : Action

Starts image capture or video recording depending on the Mode. If there is a capture already going on, does nothing. Resumes video recording if it has been paused.

`camera` : | the camera bin element
`user_data` : | user data set when the signal handler was connected.

### The `"capture-stop"` signal

    void                user_function                      (GstCameraBin *camera,
                                                            gpointer      user_data)      : Action

Stops still image preview, continuous image capture and video recording and returns to the view finder mode.

`camera` : | the camera bin element
`user_data` : | user data set when the signal handler was connected.

### The `"image-done"` signal

    gboolean            user_function                      (GstCameraBin *camera,
                                                            gchar        *filename,
                                                            gpointer      user_data)      : Run Last

Signal emitted when the file has just been saved.

Don't call any GstCameraBin method from this signal, if you do so there will be a deadlock.

`camera` : | the camera bin element
`filename` : | the name of the file just saved
`user_data` : | user data set when the signal handler was connected.

### The `"set-image-resolution"` signal

    void                user_function                      (GstCameraBin *camera,
                                                            gint          width,
                                                            gint          height,
                                                            gpointer      user_data)      : Action

Changes the resolution used for still image capture. Does not affect view finder mode and video recording.

This actually sets the 'image-capture-width' and 'image-capture-height' properties.

`camera` : | the camera bin element
`width` : | number of horizontal pixels
`height` : | number of vertical pixels
`user_data` : | user data set when the signal handler was connected.

### The `"set-video-resolution-fps"` signal

    void                user_function                      (GstCameraBin *camera,
                                                            gint          width,
                                                            gint          height,
                                                            gint          fps_n,
                                                            gint          fps_d,
                                                            gpointer      user_data)      : Action

Changes the frame resolution and frames per second of the video source. The application must be aware of the resolutions supported by the camera. Supported resolutions and frame rates can be get using input-caps property.

Setting `fps_n` or `fps_d` to 0 configures maximum framerate for the given resolution, unless in night mode when minimum is configured.

This is the same as setting the 'video-capture-width', 'video-capture-height' and 'video-capture-framerate' properties, but it already updates the caps to force use this resolution and framerate.

`camera` : | the camera bin element
`width` : | number of horizontal pixels
`height` : | number of vertical pixels
`fps_n` : | frames per second numerator
`fps_d` : | frames per second denominator
`user_data` : | user data set when the signal handler was connected.