## gstbasertppayload gstbasertppayload — Base class for RTP payloader |

## Synopsis

    #include <gst/rtp/gstbasertppayload.h>

    struct              GstBaseRTPPayload;
    struct              GstBaseRTPPayloadClass;
    #define             GST_BASE_RTP_PAYLOAD_MTU            (payload)
    #define             GST_BASE_RTP_PAYLOAD_PT             (payload)
    #define             GST_BASE_RTP_PAYLOAD_SINKPAD        (payload)
    #define             GST_BASE_RTP_PAYLOAD_SRCPAD         (payload)
    gboolean            gst_basertppayload_is_filled        (GstBaseRTPPayload *payload,
                                                             guint size,
                                                             GstClockTime duration);
    GstFlowReturn       gst_basertppayload_push             (GstBaseRTPPayload *payload,
                                                             GstBuffer *buffer);
    GstFlowReturn       gst_basertppayload_push_list        (GstBaseRTPPayload *payload,
                                                             GstBufferList *list);
    void                gst_basertppayload_set_options      (GstBaseRTPPayload *payload,
                                                             const gchar *media,
                                                             gboolean dynamic,
                                                             const gchar *encoding_name,
                                                             guint32 clock_rate);
    gboolean            gst_basertppayload_set_outcaps      (GstBaseRTPPayload *payload,
                                                             const gchar *fieldname,
                                                             ...);

## Object Hierarchy

      GObject
       +----GstObject
             +----GstElement
                   +----GstBaseRTPPayload
                         +----GstBaseRTPAudioPayload

## Properties

      "max-ptime"                gint64                : Read / Write
      "min-ptime"                gint64                : Read / Write
      "mtu"                      guint                 : Read / Write
      "perfect-rtptime"          gboolean              : Read / Write
      "pt"                       guint                 : Read / Write
      "ptime-multiple"           gint64                : Read / Write
      "seqnum"                   guint                 : Read
      "seqnum-offset"            gint                  : Read / Write
      "ssrc"                     guint                 : Read / Write
      "timestamp"                guint                 : Read
      "timestamp-offset"         guint                 : Read / Write

## Description

Provides a base class for RTP payloaders

## Details

### struct GstBaseRTPPayload

    struct GstBaseRTPPayload;

### struct GstBaseRTPPayloadClass

    struct GstBaseRTPPayloadClass {
      GstElementClass parent_class;

      /* receive caps on the sink pad, configure the payloader. */
      gboolean      (*set_caps)             (GstBaseRTPPayload *payload, GstCaps *caps);
      /* handle a buffer, perform 0 or more gst_basertppayload_push() on
       * the RTP buffers. This function takes ownership of the buffer. */
      GstFlowReturn (*handle_buffer)        (GstBaseRTPPayload *payload,
                                             GstBuffer *buffer);
      gboolean      (*handle_event)         (GstPad * pad, GstEvent * event);
      GstCaps *     (*get_caps)             (GstBaseRTPPayload *payload, GstPad * pad);
    };

### GST_BASE_RTP_PAYLOAD_MTU()

    #define GST_BASE_RTP_PAYLOAD_MTU(payload) (GST_BASE_RTP_PAYLOAD (payload)->mtu)

Get access to the configured MTU of `payload`.

`payload` : | a GstBaseRTPPayload

### GST_BASE_RTP_PAYLOAD_PT()

    #define GST_BASE_RTP_PAYLOAD_PT(payload)  (GST_BASE_RTP_PAYLOAD (payload)->pt)

Get access to the configured payload type of `payload`.

`payload` : | a GstBaseRTPPayload

### GST_BASE_RTP_PAYLOAD_SINKPAD()

    #define GST_BASE_RTP_PAYLOAD_SINKPAD(payload) (GST_BASE_RTP_PAYLOAD (payload)->sinkpad)

Get access to the sinkpad of `payload`.

`payload` : | a GstBaseRTPPayload

### GST_BASE_RTP_PAYLOAD_SRCPAD()

    #define GST_BASE_RTP_PAYLOAD_SRCPAD(payload)  (GST_BASE_RTP_PAYLOAD (payload)->srcpad)

Get access to the srcpad of `payload`.

`payload` : | a GstBaseRTPPayload

### gst_basertppayload_is_filled ()

    gboolean            gst_basertppayload_is_filled        (GstBaseRTPPayload *payload,
                                                             guint size,
                                                             GstClockTime duration);

Check if the packet with `size` and `duration` would exceed the configured maximum size.

`payload` : | a GstBaseRTPPayload
`size` : | the size of the packet
`duration` : | the duration of the packet
Returns : | `TRUE` if the packet of `size` and `duration` would exceed the configured MTU or max_ptime.

### gst_basertppayload_push ()

    GstFlowReturn       gst_basertppayload_push             (GstBaseRTPPayload *payload,
                                                             GstBuffer *buffer);

Push `buffer` to the peer element of the payloader. The SSRC, payload type, seqnum and timestamp of the RTP buffer will be updated first.

This function takes ownership of `buffer`.

`payload` : | a GstBaseRTPPayload
`buffer` : | a GstBuffer
Returns : | a GstFlowReturn.

### gst_basertppayload_push_list ()

    GstFlowReturn       gst_basertppayload_push_list        (GstBaseRTPPayload *payload,
                                                             GstBufferList *list);

Push `list` to the peer element of the payloader. The SSRC, payload type, seqnum and timestamp of the RTP buffer will be updated first.

This function takes ownership of `list`.

`payload` : | a GstBaseRTPPayload
`list` : | a GstBufferList
Returns : | a GstFlowReturn.

Since 0.10.24

### gst_basertppayload_set_options ()

    void                gst_basertppayload_set_options      (GstBaseRTPPayload *payload,
                                                             const gchar *media,
                                                             gboolean dynamic,
                                                             const gchar *encoding_name,
                                                             guint32 clock_rate);

Set the rtp options of the payloader. These options will be set in the caps of the payloader. Subclasses must call this method before calling `gst_basertppayload_push()` or `gst_basertppayload_set_outcaps()`.

`payload` : | a GstBaseRTPPayload
`media` : | the media type (typically "audio" or "video")
`dynamic` : | if the payload type is dynamic
`encoding_name` : | the encoding name
`clock_rate` : | the clock rate of the media

### gst_basertppayload_set_outcaps ()

    gboolean            gst_basertppayload_set_outcaps      (GstBaseRTPPayload *payload,
                                                             const gchar *fieldname,
                                                             ...);

Configure the output caps with the optional parameters.

Variable arguments should be in the form field name, field type (as a GType), value(s). The last variable argument should be NULL.

`payload` : | a GstBaseRTPPayload
`fieldname` : | the first field name or `NULL`
`...` : | field values
Returns : | `TRUE` if the caps could be set.

## Property Details

### The `"max-ptime"` property

      "max-ptime"                gint64                : Read / Write

Maximum duration of the packet data in ns (-1 = unlimited up to MTU).

Allowed values: >= -1

Default value: -1

### The `"min-ptime"` property

      "min-ptime"                gint64                : Read / Write

Minimum duration of the packet data in ns (can't go above MTU).

Allowed values: >= 0

Default value: 0

### The `"mtu"` property

      "mtu"                      guint                 : Read / Write

Maximum size of one packet.

Allowed values: >= 28

Default value: 1400

### The `"perfect-rtptime"` property

      "perfect-rtptime"          gboolean              : Read / Write

Generate perfect RTP timestamps when possible.

Default value: TRUE

### The `"pt"` property

      "pt"                       guint                 : Read / Write

The payload type of the packets.

Allowed values: <= 128

Default value: 96

### The `"ptime-multiple"` property

      "ptime-multiple"           gint64                : Read / Write

Force buffers to be multiples of this duration in ns (0 disables).

Allowed values: >= 0

Default value: 0

### The `"seqnum"` property

      "seqnum"                   guint                 : Read

The RTP sequence number of the last processed packet.

Allowed values: <= 65535

Default value: 0

### The `"seqnum-offset"` property

      "seqnum-offset"            gint                  : Read / Write

Offset to add to all outgoing seqnum (-1 = random).

Allowed values: [G_MAXULONG,65535]

Default value: -1

### The `"ssrc"` property

      "ssrc"                     guint                 : Read / Write

The SSRC of the packets (default == random).

Default value: 4294967295

### The `"timestamp"` property

      "timestamp"                guint                 : Read

The RTP timestamp of the last processed packet.

Default value: 0

### The `"timestamp-offset"` property

      "timestamp-offset"         guint                 : Read / Write

Offset to add to all outgoing timestamps (default = random).

Default value: 4294967295